netXSer Driver Version History:

V6.0.9.0 (15.07.2013)
---------------------
 - System may not respond anymore (hang) under special conditions

V6.0.8.0 (21.06.2013)
---------------------
 - COM Port may be opened simultaneously by multiple applications
 - [Windows 8] COM Port can only by opened by applications running as administrators

V6.0.7.0 (01.10.2012)
---------------------
 - Disconnecting USB Device during transfer (e.g. xSysdeviceReset) may result in Blue Screen or system hang
 - netRAPID10 added

V6.0.6.0 (26.07.2012)
---------------------
 - Updated INF file for netX10 devices

V6.0.5.0 (24.02.2011)
---------------------
 - Reduced send frame size to 63 bytes as netX10 gets stuck sometimes when using
   full 64 byte frames

V6.0.4.0 (21.02.2011)
---------------------
 - Incorrect name displayed for COMX10 
 - Additional Driver Interfaces removed due to timeout problems with netXTransport.dll

V6.0.3.0 (12.12.2011)
---------------------
 - Driver may cause blue screen after trying to reconnect to a previously closed
   COM port

V6.0.2.0 (02.12.2011)
---------------------
 - Removed support for ROM Loader, which is handled via libusb using the bootwizard tool
 - Added special half-duplex protocol to work around a bug in the netX10 USB core
   (needs 2nd Stage Loader V1.4.5.0 or later)

V6.0.1.0 (internal test version, not released)
----------------------------------------------
 Bugfix:
  - Incoming data may not be provided if the last frame has a length of 64 Bytes.
    Reader Pipe is now used with 64 Byte frames every 1ms, as netX10 does not provide
    a ZLP as end of transfer packet.

    NOTE: This fix will only be enabled for netX10 ROM Loader.

V6.0.0.0 (16.09.2010)
---------------------
 - initial version

NOTE: V6.0.0.0 was chosen as the current HilUsbSer.sys uses V5.X.X.X and this 
      driver must be able to replace HilUsbSer.sys for netX10.
