;=======================================================
; B2410WE.INF Ver. 1.0 06/18/2021
;
; Monitor INF file for Fujitsu Display B2410 WE
;
; Copyright 2021 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FTS-Mfg%
CatalogFile = B2410WE.cat
DriverVer   = 06/18/2021, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
B2410WE.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
B2410WE.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS08F4
ExcludeFromSelect = Monitor\FUS08F5
ExcludeFromSelect = Monitor\FUS08F6
ExcludeFromSelect = Monitor\FUS08F7

[Manufacturer]
%FTS-Mfg% = FTS-Mfg, NTx86, NTAMD64

[FTS-Mfg]
%B2410WE.VGA%  = B2410WE.VGA.Install, Monitor\FUS08F4
%B2410WE.DVI%  = B2410WE.DVI.Install, Monitor\FUS08F5
%B2410WE.HDMI%  = B2410WE.HDMI.Install, Monitor\FUS08F6
%B2410WE.DP%     = B2410WE.DP.Install, Monitor\FUS08F7

[FTS-Mfg.NTx86]
%B2410WE.VGA%  = B2410WE.VGA.Install, Monitor\FUS08F4
%B2410WE.DVI%  = B2410WE.DVI.Install, Monitor\FUS08F5
%B2410WE.HDMI%  = B2410WE.HDMI.Install, Monitor\FUS08F6
%B2410WE.DP%     = B2410WE.DP.Install, Monitor\FUS08F7

[FTS-Mfg.NTAMD64]
%B2410WE.VGA%  = B2410WE.VGA.Install, Monitor\FUS08F4
%B2410WE.DVI%  = B2410WE.DVI.Install, Monitor\FUS08F5
%B2410WE.HDMI%  = B2410WE.HDMI.Install, Monitor\FUS08F6
%B2410WE.DP%     = B2410WE.DP.Install, Monitor\FUS08F7

[B2410WE.VGA.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = B2410WE.VGA.AddReg, 1920x1200, DPMS
CopyFiles = B2410WE.CopyFiles

[B2410WE.DVI.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = B2410WE.DVI.AddReg, 1920x1200, DPMS
CopyFiles = B2410WE.CopyFiles

[B2410WE.HDMI.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = B2410WE.HDMI.AddReg, 1920x1200, DPMS
CopyFiles = B2410WE.CopyFiles

[B2410WE.DP.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = B2410WE.DP.AddReg, 1920x1200, DPMS
CopyFiles = B2410WE.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[B2410WE.VGA.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,48-76,+,-"
HKR,,ICMProfile,0,"B2410WE.icm"

[B2410WE.DVI.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,48-76,+,-"
HKR,,ICMProfile,0,"B2410WE.icm"

[B2410WE.HDMI.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,48-76,+,-"
HKR,,ICMProfile,0,"B2410WE.icm"

[B2410WE.DP.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,48-76,+,-"
HKR,,ICMProfile,0,"B2410WE.icm"

[1920x1200]
HKR,,MaxResolution,,"1920,1200"

[DPMS]
HKR,,DPMS,,1

[B2410WE.CopyFiles]
B2410WE.icm

[B2410WE.VGA.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[B2410WE.DVI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[B2410WE.HDMI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[B2410WE.DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FTS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

B2410WE.VGA = "Fujitsu B2410 WE (VGA)"
B2410WE.DVI = "Fujitsu B2410 WE (DVI)"
B2410WE.HDMI= "Fujitsu B2410 WE (HDMI)"
B2410WE.DP  = "Fujitsu B2410 WE (DP)"
